# Theatr Clwyd

# Emlyn Williams Theatre - Technical Overview.

## Auditorium.

* Flexible studio space
* Freestanding, upholstered seating on steeldeck rostra, can be arranged in many formats. Plans of standard layouts available on website.
* Capacity in the range 147 - 250 depending on layout.
* Visiting companies normally use one of two possible end stage arrangement, giving either 167 seats with 7m full height stage depth, or 147 seats with 8m stage depth.
* Lighting / seating balcony round sides can give up to 20 extra seats.
* Control and viewing rooms at balcony level.

## Stage.

* Total Floor area 16m x 16m; performing area variable between 5m x 5m to 7m x 16m.
* Wing space formed within floor area by layout.
* Access to all corners of space from outside.
* Lighting / seating balcony on three sides, 1m wide, 3.24m clearance under. Control Room takes up part of balcony on one side.
* 3 x Winch bars for cloths, cyc, blacks etc. across north wall (opposite control room wall).
* Prompt Desk normally in control room; can be at floor level.
* Get in at stage level; twin loading bay, each door 2.75m x 3.1m, then via double door 1.6m wide x 3.1m high

## Lighting and Sound.

See separate plans and schedules.

## Dressing rooms.

* Four at balcony level, accommodating 15, all with shower.
* Toilets at stage and balcony level.
* Disabled toilet at stage level, Green Room with catering service, and bathroom, all shared with Anthony Hopkins Theatre.
* Coin-operated launderette machines available.