# Theatr Clwyd

# Antony Hopkins Theatre - Technical Overview .

## Auditorium.

* Single raked tier, continental seating, 519 seats + 5 wheelchair spaces.
* Forestage lifts can give extra 45 Seats.
* Control, projection and viewing rooms at rear.

## Stage.

* Proscenium stage; opening 10.65metres x 6.5m high (variable).
* Safety Curtain to back wall 10.74 metres.
* Safety Curtain to front of stage 1.11 metres.
* Front of stage to front of forestage 3.72 metres.
* Flat stage, sprung hardwood floor, hardboard surface.
* Carpet cuts, footlight troughs, and trapdoors in stage floor, normally hardboarded over.
* Wing widths 8 metres SR, 2.5 metres SL.
* 59 single purchase counterweight sets SL (inc 2 up & down).
* Grid height 18.48m
* Forestage lifts can give orchestra pit for 40.
* Bosendorfer Imperial grand piano.
* Prompt Corner SL.
* Get in at stage level; twin loading bay, each door 2.75m high x 3.1m.

## Lighting and Sound.

See separate plans and schedules.

## Dressing rooms.

* Six at stage level, accommodating 24, all with shower.
* (DR4 for 4, DR5 for 5, DR6 for 3, DR7 for 3, DR8 for 5, DR9 for 4)
* Toilets and disabled toilet at stage level.
* Visiting company office.
* Green Room with catering service on first floor.
* Bathroom on first floor.
* Two band rooms below stage.
* Coin-operated launderette machines available.